{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["多媒体教室设备"],"read":"whole","date_system":"1900"}

{"sheet":"多媒体教室设备","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"merged":[[0,0,0,5],[1,0,2,0],[1,1,2,1],[1,3,2,3],[1,5,2,5],[3,0,4,0],[3,1,4,1],[3,3,4,3],[3,4,4,4],[3,5,4,5],[5,0,6,0],[5,1,6,1],[5,3,6,3],[5,4,6,4],[5,5,6,5],[7,0,10,0],[7,1,10,1],[7,3,10,3],[7,4,10,4],[7,5,10,5],[8,2,10,2],[11,0,16,0],[11,1,16,1],[11,3,16,3],[11,4,16,4],[11,5,13,5],[12,2,16,2],[17,0,21,0],[17,1,21,1],[17,3,21,3],[17,4,21,4],[17,5,18,5],[18,2,21,2],[22,0,26,0],[22,1,26,1],[22,3,26,3],[22,4,26,4],[22,5,23,5],[23,2,26,2],[27,0,28,0],[27,1,28,1],[27,3,28,3],[27,4,28,4],[27,5,28,5]]}
["微格教学实训器材项目相关技术参数要求"]
["序号","名称","品牌","技术参数","单","数量"]
[null,null,"型号",null,"位"]
[1,"Sony/索尼 ILCE-6400L + 18-105mm f4 G镜头","SONY","2420万有效像素，ExmorCMOS影像传感器，ISO100-32000可扩展102400，425个相位检测自动对焦点，0.02秒快速对焦，11张/秒高速连拍，实时眼部对焦，实时追踪功能，4K HDR视频，180度可翻折触摸屏","台",1]
[null,null," ILCE-6400L"]
[2,"球形直播LED通用灯笼罩","神牛","高透度材质制作、360度透光，柔光效果出众，可以实行光线照射由中心到边缘，由高光中心点逐渐减弱的光影变化。适用于SL150太阳灯，所见即所得，光线非常柔和，色彩饱和度高，照明范围：2米距离光圈值可达5.6（ISO800，快门1/100S，自动白平衡）","个",2]
[null,null,"65cm"]
[3,"常亮LED视频直播补光灯","神牛","新一代COB灯珠，5600K色温，CRI>96，TLCI>97，AC电源供电：100-240V，50/60Hz\n频道：16个\n组别：6组（A、B、C、D、E、F）\n功率：200W\n色温：5600K±300K（白光版SL-100W），3300K±300K（黄光版SL-100Y）\n100%光照度（LUX）：12000（1米）\n100%光通量（Lm）:20000\n显色指数（Ra值）：＞95\nR9＞70\n调光范围：10%-100%\n工作环境温度：-10-50℃\nLED灯珠安全温度：≤70℃纠错","个",3]
[null,null,"200W"]
[]
[]
[4,"摄影大力夹 ","神牛","应用于影视和摄影拍摄中，夹背景布、背景纸、反光板和柔光纸等各类物品。","个",6]
[null,null,"8cm大力夹"]
[]
[]
[]
[]
[5,"LED500II双色温白光户外拍摄像视频单反平板直播摄影灯","神牛","变色版LED500LC，300-5600K，252颗灯珠，光照亮度：2900，功率：32W，250mmX170mmX45mm","个",1]
[null,null,"32W"]
[]
[]
[]
[6,"收音话筒杆伸缩杆","博雅","挑杆规格：四方杆，材质：铝合金，长度：3.8米，承重：3kg，","根",1]
[null,null,"3.8米"]
[]
[]
[]
[7,"麦克风Vlog视频采访Wirelessgo录音","RODE罗德","品牌：Rode 产品类型：麦克风/话筒 型号：wireless go 2(WIRELESS GO II)\n用途：直播show 传输方式：无线 连接主体：笔记本,相机/摄像机\n供电方式：内置电池 使用方式：领夹式 读取方式：OTG","套",1]
[null,null,"Wireless GO II 一拖二采访套装"]